 ****** HSPICE -Z-2007.03 32-BIT  (Feb 28 2007) 17:33:17 02/22/2009 pcnt       
  Copyright (C) 2007 Synopsys, Inc. All Rights Reserved.                       
  Unpublished-rights reserved under US copyright laws.
  This program is protected by law and is subject to the 
  terms and conditions of the license agreement found in:
    C:\synopsys\Hspice_Z-2007.03\license.txt
  Use of this program is your acceptance to be bound by this 
  license agreement. HSPICE is the trademark of Synopsys, Inc.
  Input File: s:\87-88-1\qz\data_converter\project\help2\dac.sp                 
  lic:  
  lic: FLEXlm: v8.4b 
  lic: USER:   shamsi               HOSTNAME: DrShamsi 
  lic: HOSTID: 001a4d85f8fc         PID:      3044 
  lic: Using FLEXlm license file: 
  lic: C:\synopsys\V-2004.06-SP1\Saber\licensing\saber.lic 
  lic: Using FLEXlm license file: 
  lic: C:\synopsys\V-2004.06-SP1\Saber\licensing\saber.lic 
  lic: Unable to checkout hspice 
  lic:   
  lic:  
  lic: FLEXlm: v8.4b 
  lic: USER:   shamsi               HOSTNAME: DrShamsi 
  lic: HOSTID: 001a4d85f8fc         PID:      3044 
  lic: Using FLEXlm license file: 
  lic: C:\synopsys\V-2004.06-SP1\Saber\licensing\saber.lic 
  lic: Using FLEXlm license file: 
  lic: C:\synopsys\V-2004.06-SP1\Saber\licensing\saber.lic 
  lic: Unable to checkout hspicewin 
  lic:   
 Init: read install configuration file: C:\synopsys\Hspice_Z-2007.03\meta.cfg
  Init: hspice initialization file: C:\synopsys\Hspice_Z-2007.03\hspice.ini     
                                                  
 vb5     b5    0    pwl  (t,bsig5  )
 vb5b    b5b   0    pwl  (t,bsig5b )   
 vb5b    b5b   0    pwl  (t,bsig5b )   
 vb6     b6    0    pwl  (t,bsig6  )   
 vb6     b6    0    pwl  (t,bsig6  )   
 vb6b    b6b   0    pwl  (t,bsig6b )   
 vb6b    b6b   0    pwl  (t,bsig6b )   
 vb7     b7    0    pwl  (t,bsig7  )   
 vb7     b7    0    pwl  (t,bsig7  )   
 vb7b    b7b   0    pwl  (t,bsig7b )   
 vb7b    b7b   0    pwl  (t,bsig7b )   
 vb8     b8    0    pwl  (t,bsig8  )   
 vb8     b8    0    pwl  (t,bsig8  )   
 vb8b    b8b   0    pwl  (t,bsig8b )   
 vb8b    b8b   0    pwl  (t,bsig8b )   
 vb9     b9    0    pwl  (t,bsig9  )   
 vb9     b9    0    pwl  (t,bsig9  )   
 vb9b    b9b   0    pwl  (t,bsig9b )   
 vb9b    b9b   0    pwl  (t,bsig9b )   
 vb10    b10   0    pwl  (t,bsig10 )   
 vb10    b10   0    pwl  (t,bsig10 )   
 vb10b   b10b  0    pwl  (t,bsig10b)   
 vb10b   b10b  0    pwl  (t,bsig10b)   

 vd1     d1    0    pwl  (t,dsig1  )   
 vd1b    d1b   0    pwl  (t,dsig1b )
 vd1b    d1b   0    pwl  (t,dsig1b )
 vd2     d2    0    pwl  (t,dsig2  )   
 vd2     d2    0    pwl  (t,dsig2  )   
 vd2b    d2b   0    pwl  (t,dsig2b )
 vd2b    d2b   0    pwl  (t,dsig2b )
 vd3     d3    0    pwl  (t,dsig3  )   
 vd3     d3    0    pwl  (t,dsig3  )   
 vd3b    d3b   0    pwl  (t,dsig3b )
 vd3b    d3b   0    pwl  (t,dsig3b )
 vd4     d4    0    pwl  (t,dsig4  )   
 vd4     d4    0    pwl  (t,dsig4  )   
 vd4b    d4b   0    pwl  (t,dsig4b )
 vd4b    d4b   0    pwl  (t,dsig4b )
 vd5     d5    0    pwl  (t,dsig5  )   
 vd5     d5    0    pwl  (t,dsig5  )   
 vd5b    d5b   0    pwl  (t,dsig5b )
 vd5b    d5b   0    pwl  (t,dsig5b )
 vd6     d6    0    pwl  (t,dsig6  )   
 vd6     d6    0    pwl  (t,dsig6  )   
 vd6b    d6b   0    pwl  (t,dsig6b )
 vd6b    d6b   0    pwl  (t,dsig6b )
 vd7     d7    0    pwl  (t,dsig7  )   
 vd7     d7    0    pwl  (t,dsig7  )   
 vd7b    d7b   0    pwl  (t,dsig7b )
 vd7b    d7b   0    pwl  (t,dsig7b )
 vd8     d8    0    pwl  (t,dsig8  )
 vd8     d8    0    pwl  (t,dsig8  )
 vd8b    d8b   0    pwl  (t,dsig8b )
 vd8b    d8b   0    pwl  (t,dsig8b )
 vd9     d9    0    pwl  (t,dsig9  )   
 vd9     d9    0    pwl  (t,dsig9  )   
 vd9b    d9b   0    pwl  (t,dsig9b )
 vd9b    d9b   0    pwl  (t,dsig9b )
 vd10    d10   0    pwl  (t,dsig10 )   
 vd10    d10   0    pwl  (t,dsig10 )   
 vd10b   d10b  0    pwl  (t,dsig10b)
 vd10b   d10b  0    pwl  (t,dsig10b)
 vd11    d11   0    pwl  (t,dsig11 )   
 vd11    d11   0    pwl  (t,dsig11 )   
 vd11b   d11b  0    pwl  (t,dsig11b)
 vd11b   d11b  0    pwl  (t,dsig11b)
 vd12    d12   0    pwl  (t,dsig12 )   
 vd12    d12   0    pwl  (t,dsig12 )   
 vd12b   d12b  0    pwl  (t,dsig12b)
 vd12b   d12b  0    pwl  (t,dsig12b)
 vd13    d13   0    pwl  (t,dsig13 )   
 vd13    d13   0    pwl  (t,dsig13 )   
 vd13b   d13b  0    pwl  (t,dsig13b)
 vd13b   d13b  0    pwl  (t,dsig13b)
 vd14    d14   0    pwl  (t,dsig14 )   
 vd14    d14   0    pwl  (t,dsig14 )   
 vd14b   d14b  0    pwl  (t,dsig14b)
 vd14b   d14b  0    pwl  (t,dsig14b)
 vd15    d15   0    pwl  (t,dsig15 )   
 vd15    d15   0    pwl  (t,dsig15 )   
 vd15b   d15b  0    pwl  (t,dsig15b)
 vd15b   d15b  0    pwl  (t,dsig15b)

 .tran data=pwl_sig
 .option post ingold=2 numdgt=10 delmax=100p method=gear accurate=1
 .option post ingold=2 numdgt=10 delmax=100p method=gear accurate=1
 .op
 .op

  **warning** (mm018.l:503)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:564)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:627)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:693)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:755)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:820)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:886)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:948)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1010)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1076)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1139)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1203)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1268)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1325)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1384)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1445)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1506)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1568)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1631)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1692)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1754)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1818)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1879)  associated with encrypted blocks were suppressed due to encrypted content
  **warning** (mm018.l:1940)  associated with encrypted blocks were suppressed due to encrypted content


 **warning**  the accurate option increases  the cpu time but the results
                are more accurate.
 ***accurate option sets default value of the options: 
 lvltim= 3         dvdt= 2       relvar= 200.00m absvar= 200.00m
     ft= 200.00m relmos=  10.00m
 (used for FFT control ) fft_accurate= 1

 **warning** dc voltage reset to initial transient source value
             in source        0:vb5                 new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vb5b                new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vb6                 new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vb6b                new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vb7                 new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vb7b                new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vb8                 new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vb8b                new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vb9                 new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vb9b                new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vb10                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vb10b               new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd1                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd1b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd2                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd2b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd3                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd3b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd4                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd4b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd5                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd5b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd6                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd6b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd7                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd7b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd8                 new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd8b                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd9                 new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd9b                new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd10                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd10b               new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd11                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd11b               new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd12                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd12b               new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd13                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd13b               new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd14                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd14b               new dc=  0.1800D+01


 **warning** dc voltage reset to initial transient source value
             in source        0:vd15                new dc=  0.0000D+00


 **warning** dc voltage reset to initial transient source value
             in source        0:vd15b               new dc=  0.1800D+01


 **warning** the following singular supplies were terminated to 1 meg resistor 
   supply       node1            node2
  vb10                    0:b10              defined in subckt 0                     0:0                defined in subckt 0               
  vb10b                   0:b10b             defined in subckt 0                     0:0                defined in subckt 0               
  vb5                     0:b5               defined in subckt 0                     0:0                defined in subckt 0               
  vb5b                    0:b5b              defined in subckt 0                     0:0                defined in subckt 0               
  vb6                     0:b6               defined in subckt 0                     0:0                defined in subckt 0               
  vb6b                    0:b6b              defined in subckt 0                     0:0                defined in subckt 0               
  vb7                     0:b7               defined in subckt 0                     0:0                defined in subckt 0               
  vb7b                    0:b7b              defined in subckt 0                     0:0                defined in subckt 0               
  vb8                     0:b8               defined in subckt 0                     0:0                defined in subckt 0               
  vb8b                    0:b8b              defined in subckt 0                     0:0                defined in subckt 0               
  vb9                     0:b9               defined in subckt 0                     0:0                defined in subckt 0               
  vb9b                    0:b9b              defined in subckt 0                     0:0                defined in subckt 0               
  vd1                     0:d1               defined in subckt 0                     0:0                defined in subckt 0               
  vd10                    0:d10              defined in subckt 0                     0:0                defined in subckt 0               
  vd10b                   0:d10b             defined in subckt 0                     0:0                defined in subckt 0               
  vd11                    0:d11              defined in subckt 0                     0:0                defined in subckt 0               
  vd11b                   0:d11b             defined in subckt 0                     0:0                defined in subckt 0               
  vd12                    0:d12              defined in subckt 0                     0:0                defined in subckt 0               
  vd12b                   0:d12b             defined in subckt 0                     0:0                defined in subckt 0               
  vd13                    0:d13              defined in subckt 0                     0:0                defined in subckt 0               
  vd13b                   0:d13b             defined in subckt 0                     0:0                defined in subckt 0               
  vd14                    0:d14              defined in subckt 0                     0:0                defined in subckt 0               
  vd14b                   0:d14b             defined in subckt 0                     0:0                defined in subckt 0               
  vd15                    0:d15              defined in subckt 0                     0:0                defined in subckt 0               
  vd15b                   0:d15b             defined in subckt 0                     0:0                defined in subckt 0               
  vd1b                    0:d1b              defined in subckt 0                     0:0                defined in subckt 0               
  vd2                     0:d2               defined in subckt 0                     0:0                defined in subckt 0               
  vd2b                    0:d2b              defined in subckt 0                     0:0                defined in subckt 0               
  vd3                     0:d3               defined in subckt 0                     0:0                defined in subckt 0               
  vd3b                    0:d3b              defined in subckt 0                     0:0                defined in subckt 0               
  vd4                     0:d4               defined in subckt 0                     0:0                defined in subckt 0               
  vd4b                    0:d4b              defined in subckt 0                     0:0                defined in subckt 0               
  vd5                     0:d5               defined in subckt 0                     0:0                defined in subckt 0               
  vd5b                    0:d5b              defined in subckt 0                     0:0                defined in subckt 0               
  vd6                     0:d6               defined in subckt 0                     0:0                defined in subckt 0               
  vd6b                    0:d6b              defined in subckt 0                     0:0                defined in subckt 0               
  vd7                     0:d7               defined in subckt 0                     0:0                defined in subckt 0               
  vd7b                    0:d7b              defined in subckt 0                     0:0                defined in subckt 0               
  vd8                     0:d8               defined in subckt 0                     0:0                defined in subckt 0               
  vd8b                    0:d8b              defined in subckt 0                     0:0                defined in subckt 0               
  vd9                     0:d9               defined in subckt 0                     0:0                defined in subckt 0               
  vd9b                    0:d9b              defined in subckt 0                     0:0                defined in subckt 0               
1 ****** HSPICE -Z-2007.03 32-BIT  (Feb 28 2007) 17:33:17 02/22/2009 pcnt       
 ******  
  *how to read the signal file                                                 
  ******  operating point information      tnom=  25.000 temp=  25.000         
 ******  
 ***** operating point status is all       simulation time is     0.           
    node    =voltage            node    =voltage

 +0:b10     =   0.            0:b10b    = 1.800000000e+00
 +0:b5      =   0.            0:b5b     = 1.800000000e+00
 +0:b6      =   0.            0:b6b     = 1.800000000e+00
 +0:b7      =   0.            0:b7b     = 1.800000000e+00
 +0:b8      =   0.            0:b8b     = 1.800000000e+00
 +0:b9      =   0.            0:b9b     = 1.800000000e+00
 +0:d1      = 1.800000000e+00 0:d10     =   0.           
 +0:d10b    = 1.800000000e+00 0:d11     =   0.           
 +0:d11b    = 1.800000000e+00 0:d12     =   0.           
 +0:d12b    = 1.800000000e+00 0:d13     =   0.           
 +0:d13b    = 1.800000000e+00 0:d14     =   0.           
 +0:d14b    = 1.800000000e+00 0:d15     =   0.           
 +0:d15b    = 1.800000000e+00 0:d1b     =   0.           
 +0:d2      = 1.800000000e+00 0:d2b     =   0.           
 +0:d3      = 1.800000000e+00 0:d3b     =   0.           
 +0:d4      = 1.800000000e+00 0:d4b     =   0.           
 +0:d5      = 1.800000000e+00 0:d5b     =   0.           
 +0:d6      = 1.800000000e+00 0:d6b     =   0.           
 +0:d7      = 1.800000000e+00 0:d7b     =   0.           
 +0:d8      = 1.800000000e+00 0:d8b     =   0.           
 +0:d9      =   0.            0:d9b     = 1.800000000e+00


 ****  voltage sources

 subckt                                                                      
 element        0:vb5            0:vb5b           0:vb6            0:vb6b    
  volts      0.             1.800000000e+00    0.             1.800000000e+00
  current    0.            -1.800000000e-06    0.            -1.800000000e-06
  power      0.             3.240000000e-06    0.             3.240000000e-06

 subckt                                                                      
 element        0:vb7            0:vb7b           0:vb8            0:vb8b    
  volts      0.             1.800000000e+00    0.             1.800000000e+00
  current    0.            -1.800000000e-06    0.            -1.800000000e-06
  power      0.             3.240000000e-06    0.             3.240000000e-06

 subckt                                                                      
 element        0:vb9            0:vb9b           0:vb10           0:vb10b   
  volts      0.             1.800000000e+00    0.             1.800000000e+00
  current    0.            -1.800000000e-06    0.            -1.800000000e-06
  power      0.             3.240000000e-06    0.             3.240000000e-06

 subckt                                                                      
 element        0:vd1            0:vd1b           0:vd2            0:vd2b    
  volts    1.800000000e+00    0.             1.800000000e+00    0.           
  current -1.800000000e-06    0.            -1.800000000e-06    0.           
  power    3.240000000e-06    0.             3.240000000e-06    0.           

 subckt                                                                      
 element        0:vd3            0:vd3b           0:vd4            0:vd4b    
  volts    1.800000000e+00    0.             1.800000000e+00    0.           
  current -1.800000000e-06    0.            -1.800000000e-06    0.           
  power    3.240000000e-06    0.             3.240000000e-06    0.           

 subckt                                                                      
 element        0:vd5            0:vd5b           0:vd6            0:vd6b    
  volts    1.800000000e+00    0.             1.800000000e+00    0.           
  current -1.800000000e-06    0.            -1.800000000e-06    0.           
  power    3.240000000e-06    0.             3.240000000e-06    0.           

 subckt                                                                      
 element        0:vd7            0:vd7b           0:vd8            0:vd8b    
  volts    1.800000000e+00    0.             1.800000000e+00    0.           
  current -1.800000000e-06    0.            -1.800000000e-06    0.           
  power    3.240000000e-06    0.             3.240000000e-06    0.           

 subckt                                                                      
 element        0:vd9            0:vd9b           0:vd10           0:vd10b   
  volts      0.             1.800000000e+00    0.             1.800000000e+00
  current    0.            -1.800000000e-06    0.            -1.800000000e-06
  power      0.             3.240000000e-06    0.             3.240000000e-06

 subckt                                                                      
 element        0:vd11           0:vd11b          0:vd12           0:vd12b   
  volts      0.             1.800000000e+00    0.             1.800000000e+00
  current    0.            -1.800000000e-06    0.            -1.800000000e-06
  power      0.             3.240000000e-06    0.             3.240000000e-06

 subckt                                                                      
 element        0:vd13           0:vd13b          0:vd14           0:vd14b   
  volts      0.             1.800000000e+00    0.             1.800000000e+00
  current    0.            -1.800000000e-06    0.            -1.800000000e-06
  power      0.             3.240000000e-06    0.             3.240000000e-06

 subckt                                    
 element        0:vd15           0:vd15b   
  volts      0.             1.800000000e+00
  current    0.            -1.800000000e-06
  power      0.             3.240000000e-06

     total voltage source power dissipation=  6.804000000e-05 watts



          ***** job concluded
1 ****** HSPICE -Z-2007.03 32-BIT  (Feb 28 2007) 17:33:17 02/22/2009 pcnt       
 ******  
  *how to read the signal file                                                 
  ******  job statistics summary           tnom=  25.000 temp=  25.000         
 ******  

           total memory used       8957 kbytes

  # nodes =      43 # elements=      84
  # diodes=       0 # bjts    =       0 # jfets   =       0 # mosfets =       0
  # va device =       0

    analysis           time    # points   tot. iter  conv.iter

    op point           0.00           1           3
    transient         20.32       12289     1044004      522002 rev=     49048
    readin             1.09
    errchk             0.03
    setup              0.02
    output             0.00
           total cpu time         21.49 seconds
               job started at  17:33:17 02/22/2009
               job ended   at  17:33:39 02/22/2009


  Init: hspice initialization file: C:\synopsys\Hspice_Z-2007.03\hspice.ini     
                                                  
